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iCerMax™ 1” Diesel filter                                                  iCerMax™ 1” Strainer    

-Multi pleated particle filter -   30 micron 
-Water indicator and removes water (Suspended and free water) - flow rate dependant 

Applications:
-Mobile Trailers
-Famers Gravity tanks
-Filling Gensec tanks on receiving 
-inline Strainers 
-Small kerbside pumps
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Use as inline Strainer to protect pumps, especially at tank cleaning:
[bookmark: _GoBack]-1” flow, no internal reduction on flow, no cavitation on pump, especially fitted on suction side,   
   other products reduce to 14 mm inside, cause cavitation on pump 
- Clear bowl visible 
- Red ball water indicator 
- Metal strainer reusable - 150 micron 
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